// Copyright (c) 2005 DMTF.  All rights reserved.
// <change cr="SysDevCR00722.000" type ="change">Update of
// descriptions based on Tech Edit review.</
// <change cr="ArchCR00066.004" type="add">Add UmlPackagePath
// qualifier values to CIM Schema.</change>
// ==================================================================
//  CIM_RemotePort
// ==================================================================
   [Version ( "2.10.0" ), 
    UMLPackagePath ( "CIM::Core::Service" ), 
    Description ( 
       "RemotePort adds port information to the access data (such as "
       "IP Address) that is specified in and inherited from "
       "RemoteServiceAccessPoint. For example, using the additional "
       "properties in this class, you could indicate that UDP Port 123 "
       "is accessed at IP Address xyz. The IP Address would be "
       "specified in the inherited AccessInfo property, while the UDP "
       "Port number would be specified in the PortInfo property of "
       "this class." )]
class CIM_RemotePort : CIM_RemoteServiceAccessPoint {

      [Description ( 
          "Port information that might further specify the remote "
          "access information." ), 
       ModelCorrespondence { "CIM_RemotePort.PortProtocol" }]
   string PortInfo;

      [Description ( 
          "An enumerated integer that describes the protocol of the "
          "port that is addressed by PortInformation." ), 
       ValueMap { "1", "2", "3", "32768..65535" }, 
       Values { "Other", "TCP", "UDP", "Vendor Specific" }, 
       ModelCorrespondence { 
          "CIM_RemotePort.OtherProtocolDescription" }]
   uint16 PortProtocol;

      [Description ( 
          "Describes the protocol when the property PortProtocol is "
          "set to 1 (Other)." ), 
       ModelCorrespondence { "CIM_RemotePort.PortProtocol" }]
   string OtherProtocolDescription;


};
